{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["BLOCKCAL","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"BLOCKCAL","index":0,"n_rows":68,"n_cols":24,"rows_kept":68,"cut":false,"hidden":false,"merged":[[33,8,33,14],[0,20,1,20],[2,8,2,14],[2,16,2,22],[0,13,0,14],[0,16,1,16],[0,17,1,17],[0,18,1,18],[6,16,6,22],[0,11,1,11],[10,8,10,14],[16,16,16,22],[20,16,20,22],[0,19,1,19],[12,16,12,22],[5,0,6,0],[5,1,6,1],[5,2,6,2],[5,3,6,3],[5,4,6,4],[23,0,23,6],[7,0,7,6],[18,0,18,6],[22,8,22,14],[31,0,31,6],[25,8,25,14],[0,1,1,4],[0,5,0,6],[2,1,3,4],[2,5,3,5],[2,6,3,6],[5,5,5,6],[0,21,0,22],[0,8,1,8],[0,9,1,9],[0,10,1,10],[0,12,1,12]]}
[null,"Baines Masonry",null,null,null,"Load Totals",null,null,"Code","Description","Weight (kg)","No./Pal","Quantity","Total",null,null,"Code","Description","Weight (kg)","No./Pal","Quantity","Total"]
[null,null,null,null,null,"Tonne","Pallets",null,null,null,null,null,null,"Weight (kg)","Pallets",null,null,null,null,null,null,"Weight (kg)","Pallets"]
[null,"Pallet and Weight Calculator",null,null,null,{"$f":"(SUM(F9:F18)+SUM(F20:F23)+SUM(F25:F31)+SUM(F33:F37)+SUM(N4:N10)+SUM(N12:N22)+SUM(N24:N25)+SUM(N27:N33)+SUM(N35:N36)+SUM(V4:V6)+SUM(V8:V12)+SUM(V14:V16)+SUM(V19:V20)+SUM(V22))/1000","v":0},{"$f":"SUM(G9:G18)+SUM(G20:G23)+SUM(G25:G31)+SUM(G33:G37)+SUM(O4:O10)+SUM(O12:O22)+SUM(O24:O25)+SUM(O27:O33)+SUM(O35:O36)+SUM(W4:W6)+SUM(W8:W12)+SUM(W14:W16)+SUM(W19:W20)+SUM(W22)","v":0},null,"100mm Series Lightweight Betta Block",null,null,null,null,null,null,null,"Lock Block Series"]
[null,null,null,null,null,null,null,null,"10-01 BB","90mm Standard",8.83,216,0,{"$f":"K4*M4","v":0},{"$f":"IF(M4>0,M4/L4,0)","v":0},null,"LB 20-91","Standard",13.5,90,0,{"$f":"S4*U4","v":0},{"$f":"IF(U4>0,U4/T4,0)","v":0}]
[null,null,null,null,null,null,null,null,"10-02 BB","90mm 3/4",6.56,240,0,0,0,null,"LB 20-92","Cnr / End",12.06,90,0,{"$f":"S5*U5","v":0},{"$f":"IF(U5>0,U5/T5,0)","v":0}]
["Code","Description","Weight (kg)","No./Pal","Quantity","Total",null,null,"10-03 BB","90mm 1/2",4.29,360,0,0,0,null,"LB 20-93","1/2",6.72,180,0,{"$f":"S6*U6","v":0},{"$f":"IF(U6>0,U6/T6,0)","v":0}]
[null,null,null,null,null,"Weight (kg)","Pallets",null,"10-04 BB","90mm 1/4",2.33,720,0,0,0,null,"Stoneface Lock Block Series"]
["200mm Series Lightweight Betta Block",null,null,null,null,null,null,null,"10-25 BB","90mm Cnr Ret",11.07,120,0,0,0,null,"LB/SF 20-91","Standard",18,75,0,{"$f":"S8*U8","v":0},{"$f":"IF(U8>0,U8/T8,0)","v":0}]
["20-01 BB","190mm Standard",12.96,108,0,{"$f":"C9*E9","v":0},{"$f":"IF(E9>0,E9/D9,0)","v":0},null,"10-31 BB","90mm Solid",11.93,180,0,0,0,null,"LB/SF 20-92","Full Cnr / End",18,75,0,{"$f":"S9*U9","v":0},{"$f":"IF(U9>0,U9/T9,0)","v":0}]
["20-02/30-43 BB","190mm 3/4 or 290mm 1/2",9.49,144,0,0,0,null,"10-71 BB","90mm 1/2 High",4.3099999999999996,432,0,0,0,null,"LB/SF 20-93","1/2 End",10,150,0,0,0]
["20-12 BB","190mm Lintel Bond Beam",17.5,90,0,0,0,null,"150mm Series Lightweight Betta Block",null,null,null,null,null,null,null,"LB/SFD 20-92","Cnr Return",20,75,0,0,0]
["20-41/20 BB","190mm End Block",13.96,108,0,{"$f":"C12*E12","v":0},{"$f":"IF(E12>0,E12/D12,0)","v":0},null,"15-01 BB","140mm Standard",12,144,0,{"$f":"K12*M12","v":0},{"$f":"IF(M12>0,M12/L12,0)","v":0},null,"LB/SFD 20-93","1/2 Crn Return",12.5,150,0,0,0]
["20-42 BB","190mm Top Groove / Channel",12.5,108,0,0,0,null,"15-02 BB","140mm 3/4",8.19,192,0,0,0,null,"Wallaroo Sleepers"]
["20-43 BB","190mm Half End",6.97,216,0,0,0,null,"15-12 BB","140mm Lintel / bondbeam",17.440000000000001,120,0,0,0,null,"Rock","Rock Face",72,30,0,{"$f":"S14*U14","v":0},{"$f":"IF(U14>0,U14/T14,0)","v":0}]
["20-45 BB","190mm Clean Out",11.78,108,0,0,0,null,"15-20 BB","140mm Knockout bondbeam",9.7799999999999994,144,0,0,0,null,"Smooth","Smooth",72,30,0,{"$f":"S15*U15","v":0},{"$f":"IF(U15>0,U15/T15,0)","v":0}]
["20-48 BB","190mm H Block",11.68,108,0,0,0,null,"15-25 BB","140mm Cnr Ret",12.81,126,0,0,0,null,"Woodgrain","Woodgrain",72,30,0,{"$f":"S16*U16","v":0},{"$f":"IF(U16>0,U16/T16,0)","v":0}]
["20-71 BB","190mm Half High",5.98,216,0,0,0,null,"15-41 BB","140mm End Block",10.55,144,0,0,0,null,"Paver Range"]
["50-31 NAT","190mm Natural Cap",5.4,288,0,0,0,null,"15-43 BB","140mm 1/2 End ",5.4,216,0,0,0,null,"Code","Description","Weight/m2","m2/Pal","Quantity","Weight (kg)","Pallets"]
["300mm Series Lightweight Betta Block",null,null,null,null,null,null,null,"15-45 BB","140mm Clean Out",12,144,0,0,0,null,"50-33 ","Easy Paver",90,20,0,{"$f":"S19*U19","v":0},{"$f":"IF(U19>0,U19/T19,0)","v":0}]
["30-41 BB","290mm End Block",19.2,72,0,{"$f":"C20*E20","v":0},{"$f":"IF(E20>0,E20/D20,0)","v":0},null,"15-48 BB","140mm H Block",10.25,144,0,0,0,null,"60-200","Metric Paver",123.07,12.96,0,{"$f":"S20*U20","v":0},{"$f":"IF(U20>0,U20/T20,0)","v":0},"28 per M2"]
["30-42 BB","290mm Top Groove / Channel",18,72,0,{"$f":"C21*E21","v":0},{"$f":"IF(E21>0,E21/D21,0)","v":0},null,"15-71 BB","140mm 1/2 High",5.36,288,0,0,0,null,"Broughton Block",null,null,null,null,null,null,"50 per m2"]
["30-45 BB","290mm E block / Cleanout",16.45,72,0,{"$f":"C22*E22","v":0},{"$f":"IF(E22>0,E22/D22,0)","v":0},null,"15-709 FR","140mm Fire Rated",14.33,120,0,{"$f":"K22*M22","v":0},{"$f":"IF(M22>0,M22/L22,0)","v":0},null,"10-109","Broughton Edge",7,288,0,{"$f":"S22*U22","v":0},{"$f":"IF(U22>0,U22/T22,0)","v":0}]
["30-48 BB","290mm H Block",14.55,72,0,{"$f":"C23*E23","v":0},{"$f":"IF(E23>0,E23/D23,0)","v":0},null,"Abraded Face Garden Stone Series"]
["Spit Face",null,null,null,null,null,null,null,"GSB","Abraded Face Garden Stone Block",7,180,0,{"$f":"K24*M24","v":0},{"$f":"IF(M24>0,M24/L24,0)","v":0}]
["10-121","90mm Split Face Standard",12.5,144,0,{"$f":"C25*E25","v":0},{"$f":"IF(E25>0,E25/D25,0)","v":0},null,"GSC","Abraded Face Garden Stone Cap",10,180,0,{"$f":"K25*M25","v":0},{"$f":"IF(M25>0,M25/L25,0)","v":0}]
["10-123","90mm Split Face Half",6.25,288,0,0,0,null,"Retaining Wall Series"]
["15-121","140mm Split Face Standard",13,120,0,0,0,null,"020-144","Norfolk Block",18.670000000000002,90,0,{"$f":"K27*M27","v":0},{"$f":"IF(M27>0,M27/L27,0)","v":0}]
["15-123","140mm Split Face Half",6.5,240,0,0,0,null,"020-146","Norfolk Cap",22.22,90,0,{"$f":"K28*M28","v":0},0]
["20-121/142","190mm Split Face Standard",16.11,108,0,0,0,null,"225-01","Tasman Wall Block",23.33,75,0,{"$f":"K29*M29","v":0},0]
["20-123","190mm Split Face Half",8.06,216,0,0,0,null,"225-34","Tasman Full Corner",16.63,96,0,{"$f":"K30*M30","v":0},0]
["30-142","290mm Split Face Channel",22.9,72,0,0,0,null,"60-240","Tasman Full Cap",11.2,150,0,{"$f":"K31*M31","v":0},{"$f":"IF(M31>0,M31/L31,0)","v":0}]
["Coloured Smooth or Honed Blocks",null,null,null,null,null,null,null,"225-14 ","Tasman Half Corner",9.68,120,0,{"$f":"K32*M32","v":0},{"$f":"IF(M32>0,M32/L32,0)","v":0}]
["20-42/01","190mm Standard Coloured",15.59,108,0,{"$f":"C33*E33","v":0},{"$f":"IF(E33>0,E33/D33,0)","v":0},null,"60-230","Tasman Half Cap",5.35,300,0,0,{"$f":"IF(M33>0,M33/L33,0)","v":0}]
["20-03","190mm Half Coloured",7.79,216,0,{"$f":"C34*E34","v":0},{"$f":"IF(E34>0,E34/D34,0)","v":0},null,"Mine Seals"]
["50-31 ","190mm Cap Coloured",6.41,288,0,{"$f":"C35*E35","v":0},{"$f":"IF(E35>0,E35/D35,0)","v":0},null,"140-31","Mine Seal",15.63,108,0,{"$f":"K35*M35","v":0},{"$f":"IF(M35>0,M35/L35,0)","v":0}]
["15-01","140mm Standard Coloured",13.25,120,0,{"$f":"C36*E36","v":0},{"$f":"IF(E36>0,E36/D36,0)","v":0},null,"140-31DW","Dense Weight Mine Seal",16.96,108,0,{"$f":"K36*M36","v":0},0]
["10-01","90mm Standard Coloured",10.62,180,0,0,0]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,0]
[null,null,null,null,0]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}